REFER TO SUBJECT: PR10032921 COPIER PRINTER.

Copier Printer CANON IMAGE PRESS COLOR C850 COPIER/PRINTER
imagePRESS C850
MAIN ENGINE
TECHNOLOGY Electrophotography
RESOLUTION Up to 2400 x 2400 dpi
HALFTONES 256-Level Grayscale
PRINT SPEED (SIMPLEX / DUPLEX)
8.5" x 11" Up to 85 ipm
11" x 17" Up to 43 ipm
12" x 18" Up to 40 ipm
13" x 19" Up to 38 ipm
PAPER SIZE 3.94" x 5.83" to 13" x 19.2"
PAPER FEEDING
STANDARD Up to 1,650 Sheets (20 lb. Bond)
MAXIMUM Up to 7,650 Sheets (20 lb. Bond)
PAPER WEIGHT 14 lb. Bond to 110 lb. Cover (52 gsm to 300 gsm) Validated heavier stocks supported\*
ENVELOPES\*\* #10 Business, Monarch, 6" x 9", 9" x 12", 10" x 13"
DUPLEXING Automatic Duplex Any Supported Stock
POWER SOURCE Single-Phase 208 V/20 A
DIMENSIONS (H x W x D) 56.1" x 60.2" x 36.8"(Includes operator panel)
INPUT ACCESSORIES▪ ▪ ▪
MULTI-DRAWER PAPER DECK-C1
PAPER CAPACITY Up to 6,000 Sheets (20 lb. Bond)
PAPER SIZE 5.5" x 7.2" to 13" x 19.2"
PAPER WEIGHT 14 lb. Bond to 110 lb. Cover (52 gsm to 300 gsm) Validated heavier stocks supported\*
DIMENSIONS (H x W x D) 40.9" x 37.4" x 31.4"
POWER SOURCE 120 V/15 A
POD DECK LITE-C1
PAPER CAPACITY Up to 3,500 Sheets (20 lb. Bond)
PAPER SIZE 5.5" x 5.83" to 13" x 19.2"
PAPER WEIGHT 14 lb. Bond to 110 lb. Cover (52 gsm to 300 gsm) Validated heavier stocks supported\*
ENVELOPES\*\* #10 Business, Monarch, 6" x 9",9" x 12", 10" x 13"
DIMENSIONS (H x W x D) 22.5" x 28.2" x 27.0"
POWER SOURCE 120 V/15 A
STACK BYPASS-B1
PAPER CAPACITY Up to 100 Sheets (20 lb. Bond)
PAPER SIZE 3.94" x 5.83" to 13" x 19.2" (Long Sheet up to 30"\*\*\*)
PAPER WEIGHT 14 lb. Bond to 110 lb. Cover (52 gsm to 300 gsm) Validated heavier stocks supported\*
ENVELOPES #10 Business, Monarch, 6" x 9",9" x 12", 10" x 13"
DUPLEX COLOR IMAGE READER-K1
IMAGE SENSOR CCD
DOCUMENT SIZE Statement to 11" x 17"
RESOLUTION Up to 600 x 600 dpi, 256 Gradations
TRAY CAPACITY Up 300 Sheets (20 lb. Bond)
SCAN SPEED Up to 300 dpi / Up to 600 dpi
BW

https://www.usa.canon.com/internet/portal/us/home/products/details/production-printing/color-sheetfed-digital-presses/imagepress-c850

• Canon imagePRESS C850 Preferred or Equivalent specs.

• Voltage 240V