The U.S Embassy in Pretoria South Africa is requesting quotes for the supply and delivery of new vehicles.

Quote reference number: **19SF7523Q0015v1**

1. The Contractor shall supply and deliver Right-Hand Drive (RHD) motor vehicles to the U.S. Consulate, Durban, in South Africa, in accordance with the specifications and clauses set forth herein.

The contractor shall deliver vehicles that are built and homologated for export to South Africa.

Warranty shall be honored through a dealer located in Pretoria, Johannesburg, Durban and Cape Town (South Africa) with original equipment manufacturer parts for the vehicles.

Quotations / Proposals will be evaluated as a “package” to included custom cabinetry, delivery time and availability as set out in the Scope of Work (SOW) and per line item in the Solicitation.

Note: If an Offeror (s) is/are not locally registered and wanting to Import required vehicles, the Offeror (s) will not attempt to make the Embassy the importer of record. The Embassy excludes any involvement in the import process in the country of destination and cannot provide any assistance. The Offeror (s) must solicit the assistance of a local accredited Dealership.

Offerors may submit an offer for all or some of the vehicles.

The Contractor shall warrant after sale services for the vehicle (s) in South Africa.

1. This is a firm-fixed pricetype of purchase order/contract.
2. The price listed below shall include all labor, materials, overhead, profit, and transportation necessary to deliver the required items to the US Consulate in Durban, South Africa.
3. All prices from South African vendors shall be in South African Rand (ZAR). All other vendors shall price in their country currency as indicated in the pricing tables.

II. Pricing

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Line 1 | Description | Unit Price | Qty | Total Price |
| 1 | VW Transporter 6.1 Kombi 2.0 (SWB), or equivalent |  | 1 |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  | Sub Total |  |  |
|  |  | VAT |  |  |
|  |  | Grand Total |  |  |

[**Minivan**](https://en.wikipedia.org/wiki/Minivan) **/ multi-purpose vehicle (MPV) / people carrier** - Vehicle designed to transport passengers in the rear seating row(s) with reconfigurable seats in two or three rows.

[**Panel van**](https://en.wikipedia.org/wiki/Panel_van) **/ car-derived van** - A cargo vehicle based upon passenger car chassis, and typically has one row of seats with no side windows at the rear.

[**Sedan**](https://en.wikipedia.org/wiki/Sedan_(car))- A fixed-roof car in a [three-box design](https://en.wikipedia.org/wiki/Car_body_configurations#Three-box_design) with separate compartments for engine, passenger, and cargo. Sedans can have 2 or 4-doors.

**Sport utility vehicle -** A sports utility vehicle (SUV) combines elements of road-going passenger cars with features from off-road vehicles, such as raised ground clearance and four-wheel drive. There is no commonly agreed definition of an SUV, and usage varies between countries. Some definitions claim that an SUV must be built on a light truck chassis.

**LWB** – Long wheelbase

The following minimum requirements must be met:

**Vehicle Description:** VW Transporter 6.1 Kombi 2.0 (SWB), or equivalent

**Quantity:** 1

The Embassy requires the vehicle to be delivered within 90 days from date of order (PO) issued. Ex-Bonded Purchase (to excl MIDP duty Tax & Ad Valorem (Diplomatic vehicle).

* Right Hand Drive
* Platform Type:  Passenger Van

Engine and Transmission

* Fuel Type:  Diesel
* Cylinders:  4
* Minimum Engine Capacity:  2.0 Liter
* Minimum Engine Power:  110kW, or more
* Minimum Fuel Tank Capacity:  80 Liter, or more
* Transmission:  Automatic 7-Speed
* Minimum CO2 Emission: 175

Interior Features

* Minimum Seating Capacity:  8 Pax (2+3+3 configuration)
* Seat Trim:  Mesh leather in Palladium
* Floor Carpet:  Rubber floor covering with rubber mats
* Air Conditioning:  STD Climatic system (passenger compartment)
* Navigation System:  STD
* Reverse Camera: STD factory fitted.
* Audio & Communication; STD Factory fitted with 16.51” touchscreen with USB ports
* Airbags: STD factory fitted.
* Blind Spot Detection Technology (sensors)
* Powered sliding side doors

Exterior Features

* Color:  Silver / Beige
* Wheels:  17” Alloy Wheels (with full size spare wheel and full size Alloy)
* Towbar:  Yes
* Skid plates front and rear – Yes
* Mud Guards – Yes

Dimensions:

* Minimum Ground Clearance: 201mm
* Minimum Length: 5006mm
* Minimum Height: 1990mm
* Minimum Width: 1297mm
* Minimum Turning Circle: 11.9mm
* Maximum Gross (GVM): 3080

Safety Features

* Smash & Grab film fitted on all windows with maximum tint of 35%, Dealership must use an accredited fitter/installer that can provide guarantee on product.

General

* Maintenance Plan:  6 years / 180 000km
* Warranty:  3 years / 120 000 km
* Quoted price should include 21 Day South African Road Permit (the permit allows the vehicle to be transported from Dealership to Embassy without registration documents) The Embassy will do the Diplomatic registration and licensing through Foreign Affairs (DIRCO). Do NOT include registration, licensing or number plate issue fees in this quote.
* Quoted price should include Microdot (DataDot).
* Quoted price should include Road Worthiness Certificate (RWC) (if needed)
* Quoted price should include delivery costs to Durban Consulate
* Quoted price should include CO2 emissions TAX
* Quoted price should include all anticipated vehicle price increases until vehicle can be invoiced and delivered.
* Quoted price should include MIDP duty and Ad Valorem for Diplomatic purchased vehicle. (The US Embassy will provide a Certificate A for custom duties exemptions).

Delivery address

U.S. Department of State

U.S. Consulate-Durban

303 Dr. Pixley KaSeme Street

Delta Towers

30th Floor

Durban

4001